1.When the DHCP server and the WDS server are installed on the same computer, the WDS Service tries to use the port 67. However, the DHCP server already uses this port.

Wds -> properties tab->dhcp->Click to select the **Do not listen on port 67** check box, and then click **Apply**.